Assay Definition-

Assay Description:
Foolish swipes

Assay Type: DPM (Dual)
Report Name: Report1
Output Data Path: C:\Packard\Tricarb\Results\
Raw Results Path: C:\Packard\Tricarb\Results\foolish swipes\3h_14c_dpm\20120128_0837\20120128_0837.results
RTF File Name: C:\Packard\Tricarb\Results\Report1.rtf
Comma-Delimited File Name: C:\Packard\Tricarb\Results\Report1.csv
Assay File Name: C:\Packard\TriCarb\Assays\3h_14c_dpm.lsa

Additional Data Files Generated with this Protocol:
Report1
		[Excel]	Report1.csv
		[RTF]		Report1.rtf

Count Conditions-

Nuclide: 3H-14C               
   Quench Indicator: tSIE/AEC
   External Std Terminator (sec): 0.5 2s%
   Pre-Count Delay (min): 0.08
Quench Sets:                  
   Low Energy: 3H
   Mid Energy: 14C
Count Time (min): 1.00
Count Mode: Normal                                          
Assay Count Cycles: 1         Repeat Sample Count: 1        
#Vials/Sample: 1              Calculate % Reference: Off    

Background Subtract: Off
Low CPM Threshold: Off
2 Sigma % Terminator: Off

Regions         LL       UL
A              0.0     12.0
B             12.0    156.0
C              0.0      0.0

Count Corrections-

Static Controller: On         Luminescence Correction: n/a  
Colored Samples: Off          Heterogeneity Monitor: n/a    
Coincidence Time (nsec): 18   Delay Before Burst (nsec): 75 

Half Life-

Half Life Correction: Off
Regions    Half Life          Units      Reference Date      Reference Time
A                                                                          
B                                                                          
C                                                                          

Cycle 1 Results
  S#  Count Time    CPMA    CPMB    DPM1    DPM2      SIS     tSIE  MESSAGES
   1        1.00      10      23      17      27    48.47   399.77          
   2        1.00      13      44      19      53    45.88   354.25          
   3        1.00      21      26      47      29    39.94   359.07          
   4        1.00      25      12      81      10    26.35   268.79          
   5        1.00      24      55      49      64    43.89   327.59          
   6        1.00      40     105      78     124    37.53   314.21          
   7        1.00      37     163      43     198    46.55   320.32          
   8        1.00      21      26      52      28    32.01   332.38          
   9        1.00      22      29      51      33    42.63   338.13          
  10        1.00      18      33      37      38    49.61   349.54          
  11        1.00      16      61      22      73    52.85   348.23          
  12        1.00     415    1612     541    1943    47.62   341.81          
  13        1.00      61     283      59     342    60.41   356.61          
  14        1.00      27      54      55      63    43.82   341.21          
  15        1.00      24      48      48      56    45.43   343.63          
  16        1.00      46      66     103      75    39.50   345.78          
  17        1.00      19      65      27      79    58.58   347.21          
  18        1.00      18      39      34      46    54.48   351.58          
  19        1.00      11      23      23      28    45.18   294.20          
  20        1.00      21      27      54      30    35.68   297.68          
  21        1.00     102      39     282      32    20.39   323.73          
  22        1.00      20      28      44      31    44.70   364.62          
  23        1.00      27      35      68      39    31.01   307.26          
  24        1.00      26      14      70      13    28.49   327.51          
  25        1.00      79      87     204      96    32.46   307.78