Assay Definition-

Assay Description:
Foolish swipes

Assay Type: DPM (Dual)
Report Name: Report1
Output Data Path: C:\Packard\Tricarb\Results\
Raw Results Path: C:\Packard\Tricarb\Results\foolish swipes\3h_14c_dpm\20120121_0217\20120121_0217.results
RTF File Name: C:\Packard\Tricarb\Results\Report1.rtf
Comma-Delimited File Name: C:\Packard\Tricarb\Results\Report1.csv
Assay File Name: C:\Packard\TriCarb\Assays\3h_14c_dpm.lsa

Additional Data Files Generated with this Protocol:
Report1
		[Excel]	Report1.csv
		[RTF]		Report1.rtf

Count Conditions-

Nuclide: 3H-14C               
   Quench Indicator: tSIE/AEC
   External Std Terminator (sec): 0.5 2s%
   Pre-Count Delay (min): 0.08
Quench Sets:                  
   Low Energy: 3H
   Mid Energy: 14C
Count Time (min): 1.00
Count Mode: Normal                                          
Assay Count Cycles: 1         Repeat Sample Count: 1        
#Vials/Sample: 1              Calculate % Reference: Off    

Background Subtract: Off
Low CPM Threshold: Off
2 Sigma % Terminator: Off

Regions         LL       UL
A              0.0     12.0
B             12.0    156.0
C              0.0      0.0

Count Corrections-

Static Controller: On         Luminescence Correction: n/a  
Colored Samples: Off          Heterogeneity Monitor: n/a    
Coincidence Time (nsec): 18   Delay Before Burst (nsec): 75 

Half Life-

Half Life Correction: Off
Regions    Half Life          Units      Reference Date      Reference Time
A                                                                          
B                                                                          
C                                                                          

Cycle 1 Results
  S#  Count Time    CPMA    CPMB    DPM1    DPM2      SIS     tSIE  MESSAGES
   1        1.00      32      17      74      17    31.93   392.97          
   2        1.00      62      22     133      19    28.77   464.85          
   3        1.00      42      20      90      18    29.22   470.78          
   4        1.00      29      14      68      13    25.77   396.84          
   5        1.00      33      17      77      17    23.93   386.95          
   6        1.00      42      19      89      18    21.48   465.97          
   7        1.00      33      35      65      38    41.74   450.31          
   8        1.00      33      16      68      16    29.76   473.69          
   9        1.00      38      46      71      51    39.36   470.78          
  10        1.00      30      19      62      19    38.47   469.35          
  11        1.00      34      19      73      19    28.24   450.90          
  12        1.00     287     333     558     369    31.59   448.37          
  13        1.00     250     449     432     517    44.84   450.84          
  14        1.00      43      20      93      19    24.11   452.93          
  15        1.00      32      29      65      32    30.30   435.95          
  16        1.00      44      25      91      25    20.92   472.31          
  17        1.00      34      14      75      12    22.52   440.34          
  18        1.00      61      24     134      22    23.95   444.40          
  19        1.00      34      15      78      13    26.55   420.08          
  20        1.00     588     651    1272     718    28.47   384.49          
  21        1.00      37      36      73      39    38.42   467.35          
  22        1.00      59      12     133       7    17.77   441.21          
  23        1.00      33      10      76       8    22.56   426.54          
  24        1.00      76      15     168       8    17.80   463.82          
  25        1.00      71      16     186       8    16.98   359.98