Assay Definition-

Assay Description:
Foolish swipes

Assay Type: DPM (Dual)
Report Name: Report1
Output Data Path: C:\Packard\Tricarb\Results\
Raw Results Path: C:\Packard\Tricarb\Results\foolish swipes\3h_14c_dpm\20120204_1005\20120204_1005.results
RTF File Name: C:\Packard\Tricarb\Results\Report1.rtf
Comma-Delimited File Name: C:\Packard\Tricarb\Results\Report1.csv
Assay File Name: C:\Packard\TriCarb\Assays\3h_14c_dpm.lsa

Additional Data Files Generated with this Protocol:
Report1
		[Excel]	Report1.csv
		[RTF]		Report1.rtf

Count Conditions-

Nuclide: 3H-14C               
   Quench Indicator: tSIE/AEC
   External Std Terminator (sec): 0.5 2s%
   Pre-Count Delay (min): 0.08
Quench Sets:                  
   Low Energy: 3H
   Mid Energy: 14C
Count Time (min): 1.00
Count Mode: Normal                                          
Assay Count Cycles: 1         Repeat Sample Count: 1        
#Vials/Sample: 1              Calculate % Reference: Off    

Background Subtract: Off
Low CPM Threshold: Off
2 Sigma % Terminator: Off

Regions         LL       UL
A              0.0     12.0
B             12.0    156.0
C              0.0      0.0

Count Corrections-

Static Controller: On         Luminescence Correction: n/a  
Colored Samples: Off          Heterogeneity Monitor: n/a    
Coincidence Time (nsec): 18   Delay Before Burst (nsec): 75 

Half Life-

Half Life Correction: Off
Regions    Half Life          Units      Reference Date      Reference Time
A                                                                          
B                                                                          
C                                                                          

Cycle 1 Results
  S#  Count Time    CPMA    CPMB    DPM1    DPM2      SIS     tSIE  MESSAGES
   1        1.00      25      13      58      12    30.28   395.18          
   2        1.00      51     187      75     225    48.84   326.46          
   3        1.00      29      58      62      67    41.77   325.39          
   4        1.00      36      49      89      56    38.42   303.70          
   5        1.00      26      18      75      17    27.80   299.24          
   6        1.00      50      44     129      47    33.25   324.71          
   7        1.00      27      30      68      33    33.75   325.41          
   8        1.00      31      64      63      75    50.69   334.20          
   9        1.00      26      68      47      81    45.95   326.13          
  10        1.00      52      23     136      21    24.17   341.14          
  11        1.00      50     147      86     176    54.61   327.04          
  12        1.00     211    1254     107    1532    57.31   335.83          
  13        1.00      24      65      45      77    49.67   329.68          
  14        1.00      24      27      60      29    30.89   332.94          
  15        1.00      79      79     222      86    31.69   284.15          
  16        1.00      33      26      84      27    30.73   332.68          
  17        1.00      31      41      72      46    38.50   341.33          
  18        1.00      35      26      93      27    30.90   321.93          
  19        1.00      27      22      73      23    35.46   307.03          
  20        1.00      26      18      73      18    25.75   301.30          
  21        1.00      29      20      75      20    30.74   336.74          
  22        1.00      44     119      83     142    44.49   309.89          
  23        1.00      24      18      75      18    32.20   268.75          
  24        1.00      36      34      90      37    34.04   332.32